## Task 1

|  |
| --- |
| Demonstrate how to successfully configure Pexip Infinity Services |
| A screenshot showing the Pexip Connect desktop client registered successfully to an Infinity platform (notice that the boxes are greyed out, and the button at the bottom says “Unregister”): |
| A screenshot showing the Registration status on Infinity, indicating that a client has successfully registered:: |
| A screenshot of the main Live View for an inbound call to a Registered Device: |
| A screenshot of the conference graph for an inbound call to a Registered Device: |
| A screenshot of the main Live View for a call from a registered device to an external H.323 system: |
| A screenshot of the conference graph for a call from a registered device to an external H.323 system: |
| A screenshot of the main Live View for a call from a registered device to an external SIP system: |
| A screenshot of the conference graph for a call from a registered device to an external SIP system: |

## Task 2

|  |
| --- |
| Demonstrate a successful Google Meet integration for trusted and untrusted devices. |
| A screenshot of the main Live View for an untrusted Gateway instance to Google Meet: |
| A screenshot of the graph view of participants in an untrusted Gateway instance to Google Meet: |
| A screenshot of the main Live View for a trusted Gateway instance to Google Meet: |
| A screenshot of the graph view of participants in a trusted Gateway instance to Google Meet: |

## Task 3

|  |
| --- |
| Demonstrate a successful Microsoft Teams integration for trusted and untrusted devices. |
| A screenshot of the main Live View for an untrusted Gateway instance to Microsoft Teams: |
| A screenshot of the graph view of participants in an untrusted Gateway instance to Microsoft Teams: |
| A screenshot of the main Live View for a trusted Gateway instance to Microsoft Teams: |
| A screenshot of the graph view of participants in a trusted Gateway instance to Microsoft Teams: |

## Task 4

|  |
| --- |
| Demonstrate the ability to dial into Infinity from a PSTN device and transfer from a VR to a VMR. |
| A screenshot of the main Live View for a PSTN call into the general VR: |
| A screenshot of the graph view of the PSTN participant in the VR: |
| A screenshot of the main Live View for a PSTN call transferred into the VMR: |
| A screenshot of the graph view of the PSTN participant transferred into the VMR: |

## Task 5

|  |
| --- |
| Additional tasks |
|  |